

**Heater Diesel Fire 25 – Instructions for use**

**PRE-START CHECKS:**

* If using an extension lead (15m or less) it needs to be plugged directly into power.

**STARTING PROCEDURE:**

* Plug heater into power source – a green light will turn on the side of the machine.
* Push the top of the top switch on the panel IN.
* The heater will run for 20-30 seconds & will fire up on its own when ready.

**STOPPING AND AFTER USE:**

* Push the bottom of the top switch down so that it sits in the middle.
* The flame goes out & the fan continues to run for 90 seconds cooling the heater.

**SAFETY PRECAUTIONS:**

* Only use in places free of flammable vapours or high dust content.
* Ensure people & objects are kept a safe distance from the heater (3 metres).
* Keep children & animals away from the heater.
* Unplug heater when not in use.
* Ensure the heater is on a flat, stable surface.
* Only use Diesel.