**Heater Radiant Diesel Val 6– Instructions for use**

**PRE-START CHECKS:**

* You need to have sufficient space surrounding the heater at least 1.5m from the wall & the left & right side, at least 1.5m distance from the ceiling & the front side without obstacle.
* Lock the caster to avoid unexpected movement.
* Fill with diesel.

**OPERATION:**

* Plug into the power supply.
* Turn the power on.
* In order to be operated the setting temp should be hight than the current temp.
* Select temp or time control mode. You can set the desired temp between (0-40c) by pressing the “+/- “)button.

**STOPPING AND AFTER USE:**

* Turn off and unplug from the power supply.
* Leave to cool down before moving.
* Unlock the caster to move.

**SAFETY PRECAUTIONS:**

* Do not touch heater when going or immediately after use.
* Do not move the heater while it is going.
* Do not fill the heater when it is going.