**Large Gas Heater S/S – Instructions for use**

**PRE-START CHECKS:**

* Place heater in suitable position.
* Ensure LPG gas bottle is correctly connected to the heater.

**OPERATION:**

* Plug into power supply & switch on.
* Attach the heater hose to the gas bottle regulator (left hand thread) & ensure its tight.
* Open valve on gas bottle.
* Depress silver button & hold down.
* Press black button until heater starts whilst maintaining downward pressure on the silver button for 20-30 seconds.
* Release & the heater should be running.
* If flame goes out – repeat the last 2 steps.

**STOPPING AND AFTER USE:**

* Turn gas off at the bottle.
* Turn off power supply & unplug.
* Unattach the heater from the gas bottle.

**SAFETY PRECAUTIONS:**

* Do not place anything within a metre of the front of the heater.
* Do not use in enclosed space for extended periods.

**REQUIRED SAFETY EQUIPMENT:**

A black hand with a black text

Description automatically generated