**PRE-START CHECKs:**

* Thoroughly inspect area where the edger is to b used & remove any stones, sticks etc.
* Adjust blade height to suitable height.

 **Lawn Edger – Instructions for use**

**OPERATION:**

* Switch engine on.
* Slide choke lever up to full choke ON position.
* With one foot on cross brace hold down motor with left hand. With right hand pull the starter grip slowly until you feel it engage -then give it a FAST pull.
* When engine starts to run allow it to fun on half choke for a few seconds to warm up, then push choke off (down) to engine run position.
* Throttle trigger is operated by pushing down interlock with thump & pulling on trigger.
* With both arms extended downwards, hold both handle grips firmly.
* Accelerate engine by pushing down safety interlock with thumb & pulling trigger to full throttle. Blades must be spinning.
* As cutting action begins, move the lawn edger forward so that the blade can cut the edge as you move forward.

**STOPPING AND AFTER USE:**

* To stop blades rotating release the trigger.

**SAFETY PRECAUTIONS:**

* Do not lift handles by excessive bending of elbows.
* Do not operate walking backwards.
* Blades should spin under load. If blades rotate slowly, jams or stops in the ground, lower the handles & pull unit back, release trigger & recommence. Re-adjust blade hight.

**REQUIRED SAFETY EQUIPMENT:**



****