**Waterblaster on Trailer – Instructions for use**

**PRE-START CHECKs:**

* Ensure adequate water supply is available.
* Avoid kinks in suction & delivery hose.
* Remove trailer unit from tow vehicle before use & place on jockey wheel to keep level.

**OPERATION:**

* Connect water hose to blaster storage tank.
* Unwind enough pressure hose from trailer unit to move around required area.
* Turn on water supply & allow storage tank to fill.
* Leave water turned on.
* Adjust throttle to half – engage choke for cold start.
* Turn ignition switch & start.
* Return throttle to idle position & allow to warm up.
* Adjust throttle to the full position.
* Depress trigger on gun & commence cleaning.

**STOPPING AND AFTER USE:**

* Switch off machine.
* Depress trigger on gun to allow the pressure to be released.
* Disconnect all hoses & roll up.

**SAFETY PRECAUTIONS:**

* Max towing speed is 90km/hr.
* Never spray at people or animals.
* Never hold fingers or hands over high-pressure nozzle.
* Never run the machine out of water.

**REQUIRED SAFETY EQUIPMENT:**

**A black boot with text

Description automatically generated**A black hand with a black text

Description automatically generated A black headphones with text

Description automatically generated